**Vandal-resistant push-fit connector M24/125**

For wall-mounted fixed showers or shower panels

Reference: **AT821125**

Specification description

Push-fit connector M24/125 for wall-mounted fixed showers or shower panels.

For quick and easy installation of filtration devices on wall-mounted showers or a DELABIE shower panel (SPORTING, SECURITHERM, etc.). To install on a PRESTO shower panel (DL400...). we recommend an adapter (ref. AT03017).

Vandal-resistant model: tamperproof connector to avoid any vandalism or unauthorised use or removal of the filter.